# Required Components

|  |  |
| --- | --- |
| All the parts for the Gas Cap Opener laid out and numbered | **BOM**   1. Handle X2 2. Knob X2 3. Pin |

# Required Tools

* Pliers

# Required Personal Protective Equipment (PPE)

* Eye protection

# Assembly Instructions

## Step 1

Insert the octagonal pin into matching slot on one side of the handle.

|  |
| --- |
|  |

## Step 2

Align the octagonal hole on the second handle with the pin and press them together.

|  |
| --- |
|  |

## Step 3

Screw the knobs onto the threads on the handle. You may need to twist the handle slightly to align the threads. The knob will be tight, and a pair of pliers can be used to fully tighten them.

|  |
| --- |
|  |